(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 202)
    (zones 0)
    (modules 20)
    (nets 18)
  )

  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 +15V)
  (net 2 GNDA)
  (net 3 -15V)
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(RA3-Pad2)")
  (net 7 "Net-(RB3-Pad2)")
  (net 8 in_outA)
  (net 9 out_inA)
  (net 10 out_inB)
  (net 11 in_outB)
  (net 12 inB+)
  (net 13 inA+)
  (net 14 inB-)
  (net 15 inA-)
  (net 16 outA)
  (net 17 outB)

  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(RA3-Pad2)")
    (add_net "Net-(RB3-Pad2)")
    (add_net inA+)
    (add_net inA-)
    (add_net inB+)
    (add_net inB-)
    (add_net in_outA)
    (add_net in_outB)
    (add_net outA)
    (add_net outB)
    (add_net out_inA)
    (add_net out_inB)
  )

  (net_class power ""
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net -15V)
    (add_net GNDA)
  )

  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CA24E4D)
    (at 101.6 39.37)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5C54CA7D)
    (fp_text reference U1 (at 3.81 1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM4562 (at 3.81 9.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 8.95) (end 6.46 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 8.95) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 9.15) (end 8.7 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 9.15) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 in_outA))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 out_inA))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(RA3-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 in_outB))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PCIexpress_1x_letters (layer F.Cu) (tedit 5C5476B0) (tstamp 5C54794C)
    (at 96.52 66.04)
    (descr "PCIexpress Bus Edge Connector")
    (tags "PCIexpress Bus Edge Connector")
    (path /5C5482AB)
    (attr virtual)
    (fp_text reference J3 (at 5.05 -3.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x18_Row_Letter_First (at 16.48 -3.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 19.95 4.05) (end -0.95 4.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 19.95 4.05) (end 19.95 -5.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -5.45) (end -0.95 4.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -5.45) (end 19.95 -5.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 19.7 -2) (end 19.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 -2) (end 12.4 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 3.8) (end 19.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 19.7 -2) (end 12.4 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 3.8) (end -0.7 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 3.8) (end -0.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -2) (end 10.6 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -2) (end 10.6 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 -5.2) (end 12.4 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -5.2) (end 12.4 -5.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -2) (end 10.6 -5.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 9.5 0.662) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad "" connect oval (at 1 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 19 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 18 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 13 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 10 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 17 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 14 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 2 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 16 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 15 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 9 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 8 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 7 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 6 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 5 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 4 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 3 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect circle (at 1 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 17 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 16 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 15 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 14 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 13 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 0 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 10 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 9 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 8 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 7 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 6 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 5 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 4 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 3 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 2 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad 13a connect rect (at 14 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 13 inA+))
    (pad 12a connect rect (at 13 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 18a connect rect (at 19 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 12 inB+))
    (pad 17a connect rect (at 18 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 10 out_inB))
    (pad 16a connect rect (at 17 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 14 inB-))
    (pad 15a connect rect (at 16 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 15 inA-))
    (pad 14a connect rect (at 15 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 9 out_inA))
    (pad 11a connect rect (at 10 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 10a connect rect (at 9 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 9a connect rect (at 8 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 8a connect rect (at 7 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 7a connect rect (at 6 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 6a connect rect (at 5 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 5a connect rect (at 4 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 4a connect rect (at 3 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 3a connect rect (at 2 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 2a connect rect (at 1 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 1a connect rect (at 0 0) (size 0.65 3.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 13b connect rect (at 14 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 16 outA))
    (pad 12b connect rect (at 13 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 18b connect rect (at 19 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 17b connect rect (at 18 0) (size 0.65 3.6) (layers F.Cu F.Mask)
      (net 11 in_outB))
    (pad 16b connect rect (at 17 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 17 outB))
    (pad 15b connect rect (at 16 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 14b connect rect (at 15 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 8 in_outA))
    (pad 11b connect rect (at 10 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 10b connect rect (at 9 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 9b connect rect (at 8 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 8b connect rect (at 7 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 7b connect rect (at 6 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 6b connect rect (at 5 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 5b connect rect (at 4 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 4b connect rect (at 3 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 3b connect rect (at 2 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad 2b connect rect (at 1 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad 1b connect rect (at 0 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad "" connect circle (at 19 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24D4F)
    (at 96.52 54.61 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA8C)
    (fp_text reference RA2 (at -2.54 -2.54 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 inA-))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 out_inA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24B48)
    (at 91.44 44.45)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAA4)
    (fp_text reference RA3 (at 3.81 -1.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(RA3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 inA+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24BBD)
    (at 93.98 46.99 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAB9)
    (fp_text reference RA4 (at 10.16 -2.54 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10 (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24D91)
    (at 99.06 46.99 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAAC)
    (fp_text reference RA5 (at 10.16 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(RA3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24E06)
    (at 119.38 41.91 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CB19)
    (fp_text reference RB1 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 in_outB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24C29)
    (at 114.3 57.15 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAD8)
    (fp_text reference RB2 (at 1.905 -1.905 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 inB-))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24AD9)
    (at 119.38 46.99 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAE4)
    (fp_text reference RB3 (at 3.81 1.905 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(RB3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 inB+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24C6B)
    (at 116.84 49.53 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAF8)
    (fp_text reference RB4 (at 3.81 -1.92 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10 (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24CF2)
    (at 111.76 52.07 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAEC)
    (fp_text reference RB5 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66) (tstamp 5CA24DCE)
    (at 118.76 44.45 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CB0B)
    (attr virtual)
    (fp_text reference J1 (at 2.555 0 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -1.9 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 12 inB+) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66) (tstamp 5CA24B85)
    (at 92.06 41.91)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CACC)
    (attr virtual)
    (fp_text reference J2 (at 2.555 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -1.9) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 13 inA+) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 5 "Net-(J2-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24CAD)
    (at 91.44 39.37)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA95)
    (fp_text reference RA1 (at 3.81 1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 out_inA))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 in_outA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA24838)
    (at 109.18 36.83 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB2B)
    (fp_text reference C1 (at 1.23 1.905 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA24849)
    (at 104.14 49.53 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB3A)
    (fp_text reference C2 (at -2.54 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2485C)
    (at 99.06 33.655 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (path /5CA42A5F)
    (fp_text reference ClpA1 (at -3.175 0.635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330p (at 2.5 3 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -1.75) (end -1 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 1.75) (end 6 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 1.75) (end 6 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 -1.75) (end -1 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.12 -1.87) (end 6.12 -1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end -1.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.12 -1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -2) (end -1.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 2) (end 6.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 -2) (end -1.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 in_outA))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 out_inA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2486F)
    (at 111.76 36.195)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (path /5CA46ED4)
    (fp_text reference ClpB1 (at 2.5 -3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330p (at 2.5 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.25 -2) (end -1.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 2) (end 6.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -2) (end -1.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.12 -1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end -1.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end 6.12 -1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 6 -1.75) (end -1 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 1.75) (end 6 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 1.75) (end 6 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.75) (end -1 1.75) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 in_outB))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24886)
    (at 99.06 36.83 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5CA39C35)
    (fp_text reference RA7 (at -2.54 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220 (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 outA))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 in_outA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA2489D)
    (at 111.76 39.37)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5CA3D551)
    (fp_text reference RB6 (at 7.62 -1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220 (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 in_outB))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 outB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 102.52 66.54) (end 102.52 62.58) (width 0.5) (layer B.Cu) (net 1) (status 10))
  (segment (start 102.52 62.58) (end 102.87 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 104.52 62.61) (end 104.52 66.54) (width 0.5) (layer B.Cu) (net 1) (status 20))
  (segment (start 104.14 62.23) (end 104.52 62.61) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.52 66.54) (end 103.52 62.245) (width 0.5) (layer B.Cu) (net 1) (status 10))
  (segment (start 103.505 62.23) (end 104.14 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 102.87 62.23) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 102.52 63.215) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 102.52 66.54) (end 102.52 63.215) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 103.52 66.54) (end 103.52 62.245) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 104.52 63.245) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 104.52 66.54) (end 104.52 63.245) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (via (at 103.505 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 109.22 36.87) (end 109.18 36.83) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 109.22 39.37) (end 109.22 36.87) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 103.505 54.703002) (end 106.045 52.163002) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 103.505 62.23) (end 103.505 54.703002) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 106.045 52.163002) (end 106.045 40.64) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 107.315 39.37) (end 106.045 40.64) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 109.22 39.37) (end 107.315 39.37) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 104.1 49.53) (end 104.1 53.38) (width 1) (layer B.Cu) (net 2) (tstamp 5CA24D22) (status 10))
  (segment (start 104.1 53.38) (end 102.87 54.61) (width 1) (layer B.Cu) (net 2) (tstamp 5CA24D1F))
  (segment (start 99.52 66.54) (end 99.52 62.405) (width 0.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 101.52 62.785) (end 101.52 66.54) (width 0.5) (layer B.Cu) (net 2) (status 20))
  (segment (start 100.965 62.23) (end 101.52 62.785) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.52 62.675) (end 100.965 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 62.675) (width 0.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 99.695 62.23) (end 100.33 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.33 62.23) (end 100.965 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.52 63.04) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.52 66.54) (end 99.52 63.04) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 100.52 62.42) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 62.42) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 101.52 63.42) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.52 66.54) (end 101.52 63.42) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 99.52 62.405) (end 99.695 62.23) (width 0.5) (layer B.Cu) (net 2))
  (via (at 100.33 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 100.33 54.61) (end 99.06 54.61) (width 1) (layer B.Cu) (net 2) (tstamp 5CA24CDA) (status 20))
  (segment (start 93.98 54.61) (end 93.98 53.34) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C11) (status 10))
  (segment (start 95.25 52.07) (end 97.79 52.07) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C0E))
  (segment (start 93.98 53.34) (end 95.25 52.07) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C0B))
  (segment (start 99.06 53.34) (end 99.06 54.61) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C08) (status 20))
  (segment (start 97.79 52.07) (end 99.06 53.34) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C05))
  (segment (start 116.84 57.15) (end 116.84 55.88) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C02) (status 10))
  (segment (start 116.84 55.88) (end 115.57 54.61) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24BFF))
  (segment (start 99.06 60.96) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.06 54.61) (end 99.06 60.96) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 104.939999 38.570001) (end 105.880001 37.629999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 105.880001 37.629999) (end 106.68 36.83) (width 0.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 104.939999 48.730001) (end 104.939999 38.570001) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 104.14 49.53) (end 104.939999 48.730001) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 116.140001 56.450001) (end 116.84 57.15) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 115.489999 55.799999) (end 116.140001 56.450001) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 113.651999 55.799999) (end 115.489999 55.799999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 112.52 56.931998) (end 113.651999 55.799999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 112.52 66.54) (end 112.52 56.931998) (width 0.5) (layer F.Cu) (net 2))
  (via (at 101.6 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 102.87 54.61) (end 101.6 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 101.6 54.61) (end 100.33 54.61) (width 1) (layer B.Cu) (net 2))
  (via (at 105.41 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 107.95 54.61) (end 105.41 54.61) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 115.57 54.61) (end 107.95 54.61) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 107.95 54.61) (end 102.87 54.61) (width 0.5) (layer B.Cu) (net 2))
  (via (at 109.22 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 105.41 54.61) (end 109.22 54.61) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 115.52 63.013614) (end 117.573614 60.96) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 115.52 66.54) (end 115.52 63.013614) (width 0.5) (layer F.Cu) (net 2))
  (via (at 120.65 60.96) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 117.573614 60.96) (end 120.65 60.96) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 108.765001 34.744999) (end 107.479999 36.030001) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 117.456001 34.744999) (end 108.765001 34.744999) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 107.479999 36.030001) (end 106.68 36.83) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 121.049999 38.338997) (end 117.456001 34.744999) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 121.049999 60.560001) (end 121.049999 38.338997) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 120.65 60.96) (end 121.049999 60.560001) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 98.52 66.54) (end 98.52 62.325) (width 0.5) (layer B.Cu) (net 3) (status 10))
  (segment (start 98.52 62.325) (end 98.425 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 96.52 62.23) (end 96.52 66.04) (width 0.5) (layer B.Cu) (net 3) (status 20))
  (segment (start 97.52 62.595) (end 97.155 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 97.52 66.54) (end 97.52 62.595) (width 0.5) (layer B.Cu) (net 3) (status 10))
  (segment (start 97.155 62.23) (end 96.52 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 98.425 62.23) (end 97.155 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 96.52 66.54) (end 96.52 62.23) (width 0.5) (layer F.Cu) (net 3) (status 10))
  (segment (start 98.52 62.325) (end 98.52 66.54) (width 0.5) (layer F.Cu) (net 3) (status 20))
  (segment (start 98.425 62.23) (end 98.52 62.325) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.52 62.595) (end 97.52 66.54) (width 0.5) (layer F.Cu) (net 3) (status 20))
  (segment (start 97.155 62.23) (end 97.52 62.595) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.79 62.23) (end 97.155 62.23) (width 0.5) (layer F.Cu) (net 3))
  (via (at 97.79 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 3) (tstamp 5C54983B))
  (segment (start 96.52 62.23) (end 97.79 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.79 62.23) (end 98.425 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 101.6 46.99) (end 101.6 49.53) (width 1) (layer B.Cu) (net 3) (tstamp 5CA24E84) (status 30))
  (segment (start 92.629999 53.961999) (end 92.629999 55.799999) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.061998 49.53) (end 92.629999 53.961999) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 101.64 49.53) (end 97.061998 49.53) (width 0.5) (layer F.Cu) (net 3) (status 10))
  (segment (start 92.790001 55.960001) (end 97.074999 55.960001) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 92.629999 55.799999) (end 92.790001 55.960001) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.79 56.675002) (end 97.79 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.074999 55.960001) (end 97.79 56.675002) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 118.11 44.45) (end 116.84 45.72) (width 1) (layer B.Cu) (net 4) (tstamp 5CA24B27) (status 10))
  (segment (start 116.84 45.72) (end 116.84 49.53) (width 1) (layer B.Cu) (net 4) (tstamp 5CA24D34) (status 20))
  (segment (start 92.71 41.91) (end 93.98 43.18) (width 1) (layer B.Cu) (net 5) (tstamp 5CA24D31) (status 10))
  (segment (start 93.98 46.99) (end 93.98 43.18) (width 1) (layer B.Cu) (net 5) (tstamp 5CA24D2E) (status 10))
  (segment (start 119.41 46.96) (end 119.38 46.99) (width 1) (layer F.Cu) (net 12) (tstamp 5CA24D2B) (status 30))
  (segment (start 119.41 46.96) (end 119.38 46.99) (width 1) (layer B.Cu) (net 12) (tstamp 5CA24D28) (status 30))
  (segment (start 119.41 44.45) (end 119.41 46.96) (width 1) (layer B.Cu) (net 12) (tstamp 5CA24D25) (status 30))
  (segment (start 91.41 44.42) (end 91.44 44.45) (width 1) (layer B.Cu) (net 13) (tstamp 5CA24BFC) (status 30))
  (segment (start 91.41 41.91) (end 91.41 44.42) (width 1) (layer B.Cu) (net 13) (tstamp 5CA24BF9) (status 30))
  (segment (start 99.06 41.91) (end 96.52 41.91) (width 1) (layer B.Cu) (net 9) (tstamp 5CA24BF6))
  (segment (start 96.52 41.91) (end 93.98 39.37) (width 1) (layer B.Cu) (net 9) (tstamp 5CA24BF3))
  (segment (start 93.98 39.37) (end 91.44 39.37) (width 1) (layer B.Cu) (net 9) (tstamp 5CA24BF0) (status 20))
  (segment (start 101.6 41.91) (end 99.06 41.91) (width 1) (layer B.Cu) (net 9) (tstamp 5CA24BED) (status 10))
  (segment (start 96.52 46.99) (end 96.52 41.91) (width 1) (layer B.Cu) (net 9) (tstamp 5CA24BEA) (status 10))
  (segment (start 99.06 39.37) (end 101.6 39.37) (width 1) (layer B.Cu) (net 8) (tstamp 5CA24B1B) (status 30))
  (segment (start 101.6 44.45) (end 99.06 44.45) (width 1) (layer B.Cu) (net 6) (tstamp 5CA24B18) (status 30))
  (segment (start 99.06 44.45) (end 99.06 46.99) (width 1) (layer B.Cu) (net 6) (tstamp 5CA24B15) (status 30))
  (segment (start 109.22 44.45) (end 111.76 44.45) (width 1) (layer B.Cu) (net 10) (tstamp 5CA24B12) (status 10))
  (segment (start 119.38 41.91) (end 116.84 41.91) (width 1) (layer B.Cu) (net 10) (tstamp 5CA24B0F) (status 10))
  (segment (start 114.3 44.45) (end 111.76 44.45) (width 1) (layer B.Cu) (net 10) (tstamp 5CA24B0C))
  (segment (start 116.84 41.91) (end 114.3 44.45) (width 1) (layer B.Cu) (net 10) (tstamp 5CA24B09))
  (segment (start 114.3 49.53) (end 114.3 44.45) (width 1) (layer B.Cu) (net 10) (tstamp 5CA24B06) (status 10))
  (segment (start 111.76 41.91) (end 109.22 41.91) (width 1) (layer B.Cu) (net 11) (tstamp 5CA24B24) (status 30))
  (segment (start 111.76 46.99) (end 109.22 46.99) (width 1) (layer B.Cu) (net 7) (tstamp 5CA24B21) (status 30))
  (segment (start 111.76 46.99) (end 111.76 52.07) (width 1) (layer B.Cu) (net 7) (tstamp 5CA24B1E) (status 30))
  (segment (start 99.06 33.655) (end 99.06 36.83) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 99.06 36.83) (end 99.06 39.37) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 101.6 39.37) (end 102.9 39.37) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 102.9 39.37) (end 106.68 39.37) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 106.68 39.37) (end 107.315 40.005) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 107.315 40.005) (end 107.315 48.166998) (width 0.5) (layer B.Cu) (net 8))
  (via (at 107.315 49.53) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 8))
  (segment (start 107.315 48.166998) (end 107.315 49.53) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 107.315 49.53) (end 107.315 50.8) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 111.52 55.005) (end 111.52 66.54) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 107.315 50.8) (end 111.52 55.005) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 94.06 39.29) (end 93.98 39.37) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 94.06 33.655) (end 94.06 39.29) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 111.52 66.54) (end 111.52 58.18) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 110.75501 57.41501) (end 96.78501 57.41501) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 111.52 58.18) (end 110.75501 57.41501) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 92.792807 55.960001) (end 92.075 55.242194) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 95.330001 55.960001) (end 92.792807 55.960001) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 96.78501 57.41501) (end 95.330001 55.960001) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 92.075 53.972194) (end 96.52 49.527194) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 92.075 55.242194) (end 92.075 53.972194) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 96.52 49.527194) (end 96.52 46.99) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 116.76 41.83) (end 116.84 41.91) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 116.76 36.195) (end 116.76 41.83) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 114.3 52.067194) (end 114.3 49.53) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 118.190001 57.798001) (end 118.190001 55.957195) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 118.190001 55.957195) (end 114.3 52.067194) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 114.52 66.54) (end 114.52 59.47) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 114.52 59.47) (end 115.489999 58.500001) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 115.489999 58.500001) (end 117.488001 58.500001) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 117.488001 58.500001) (end 118.190001 57.798001) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 111.76 36.195) (end 111.76 39.37) (width 0.5) (layer B.Cu) (net 11))
  (segment (start 111.76 39.37) (end 111.76 41.91) (width 0.5) (layer B.Cu) (net 11))
  (segment (start 114.52 60.74) (end 114.52 63.74) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 116.935808 60.325) (end 114.935 60.325) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 114.52 63.74) (end 114.52 66.04) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 121.630011 55.630797) (end 116.935808 60.325) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 113.210001 34.744999) (end 117.456001 34.744999) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 117.456001 34.744999) (end 121.630011 38.919009) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 114.935 60.325) (end 114.52 60.74) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 111.76 36.195) (end 113.210001 34.744999) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 121.630011 38.919009) (end 121.630011 55.630797) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 115.52 61.740808) (end 115.52 66.54) (width 0.5) (layer B.Cu) (net 12))
  (segment (start 119.38 57.880808) (end 115.52 61.740808) (width 0.5) (layer B.Cu) (net 12))
  (segment (start 119.38 46.99) (end 119.38 57.880808) (width 0.5) (layer B.Cu) (net 12))
  (segment (start 95.78002 58.31502) (end 94.325011 56.860011) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 109.75002 58.31502) (end 95.78002 58.31502) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 110.52 59.085) (end 109.75002 58.31502) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 110.52 66.54) (end 110.52 59.085) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 94.325011 56.860011) (end 92.207891 56.860011) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 91.17499 55.82711) (end 92.207891 56.860011) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 91.44 45.439949) (end 91.17499 45.704959) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 91.17499 45.704959) (end 91.17499 55.82711) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 91.44 44.45) (end 91.44 45.439949) (width 0.5) (layer B.Cu) (net 13))
  (segment (start 113.52 57.93) (end 114.3 57.15) (width 0.5) (layer B.Cu) (net 14))
  (segment (start 113.52 66.54) (end 113.52 57.93) (width 0.5) (layer B.Cu) (net 14))
  (segment (start 96.52 55.599949) (end 97.435051 56.515) (width 0.5) (layer B.Cu) (net 15))
  (segment (start 96.52 54.61) (end 96.52 55.599949) (width 0.5) (layer B.Cu) (net 15))
  (segment (start 97.435051 56.515) (end 111.76 56.515) (width 0.5) (layer B.Cu) (net 15))
  (segment (start 112.52 57.275) (end 112.52 66.54) (width 0.5) (layer B.Cu) (net 15))
  (segment (start 111.76 56.515) (end 112.52 57.275) (width 0.5) (layer B.Cu) (net 15))
  (segment (start 110.52 63.74) (end 110.49 63.71) (width 0.5) (layer F.Cu) (net 16))
  (segment (start 110.52 66.54) (end 110.52 63.74) (width 0.5) (layer F.Cu) (net 16))
  (segment (start 110.49 63.71) (end 110.49 60.96) (width 0.5) (layer F.Cu) (net 16))
  (via (at 109.22 59.69) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 16))
  (segment (start 110.49 60.96) (end 109.22 59.69) (width 0.5) (layer F.Cu) (net 16))
  (segment (start 90.089999 38.180001) (end 91.44 36.83) (width 0.5) (layer B.Cu) (net 16))
  (segment (start 90.089999 56.296121) (end 90.089999 38.180001) (width 0.5) (layer B.Cu) (net 16))
  (segment (start 93.483878 59.69) (end 90.089999 56.296121) (width 0.5) (layer B.Cu) (net 16))
  (segment (start 109.22 59.69) (end 93.483878 59.69) (width 0.5) (layer B.Cu) (net 16))
  (segment (start 120.730001 55.258001) (end 116.933002 59.055) (width 0.5) (layer F.Cu) (net 17))
  (segment (start 120.730001 40.720001) (end 120.730001 55.258001) (width 0.5) (layer F.Cu) (net 17))
  (segment (start 119.38 39.37) (end 120.730001 40.720001) (width 0.5) (layer F.Cu) (net 17))
  (segment (start 116.933002 59.055) (end 114.3 59.055) (width 0.5) (layer F.Cu) (net 17))
  (segment (start 113.52 59.835) (end 113.52 66.54) (width 0.5) (layer F.Cu) (net 17))
  (segment (start 114.3 59.055) (end 113.52 59.835) (width 0.5) (layer F.Cu) (net 17))

  (zone (net 2) (net_name GNDA) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 31.75) (xy 121.92 31.75) (xy 121.92 63.5) (xy 88.9 63.5)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 31.75) (xy 121.92 31.75) (xy 121.92 63.5) (xy 88.9 63.5)
      )
    )
  )
)
