(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 37)
    (zones 0)
    (modules 20)
    (nets 28)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /relaysheet/Relais1)
  (net 2 +9V)
  (net 3 /relaysheet/Relais5)
  (net 4 /relaysheet/Relais2)
  (net 5 /relaysheet/Relais6)
  (net 6 /relaysheet/Relais3)
  (net 7 /relaysheet/Relais7)
  (net 8 /relaysheet/Relais4)
  (net 9 /relaysheet/Relais8)
  (net 10 GNDA)
  (net 11 /relaysheet/R1B_out)
  (net 12 /relaysheet/R1A_out)
  (net 13 /relaysheet/R1A_NC)
  (net 14 /relaysheet/R5B_out)
  (net 15 /relaysheet/R5A_out)
  (net 16 /relaysheet/R2B_out)
  (net 17 /relaysheet/R2A_out)
  (net 18 /relaysheet/R6A_out)
  (net 19 /relaysheet/R6B_out)
  (net 20 /relaysheet/R3A_out)
  (net 21 /relaysheet/R3B_out)
  (net 22 /relaysheet/R7B_out)
  (net 23 /relaysheet/R7A_out)
  (net 24 /relaysheet/R4A_out)
  (net 25 /relaysheet/R4B_out)
  (net 26 /relaysheet/R8A_out)
  (net 27 /relaysheet/R8B_out)

  (net_class Default "This is the default net class."
    (clearance 1)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net /relaysheet/R1A_NC)
    (add_net /relaysheet/R1A_out)
    (add_net /relaysheet/R1B_out)
    (add_net /relaysheet/R2A_out)
    (add_net /relaysheet/R2B_out)
    (add_net /relaysheet/R3A_out)
    (add_net /relaysheet/R3B_out)
    (add_net /relaysheet/R4A_out)
    (add_net /relaysheet/R4B_out)
    (add_net /relaysheet/R5A_out)
    (add_net /relaysheet/R5B_out)
    (add_net /relaysheet/R6A_out)
    (add_net /relaysheet/R6B_out)
    (add_net /relaysheet/R7A_out)
    (add_net /relaysheet/R7B_out)
    (add_net /relaysheet/R8A_out)
    (add_net /relaysheet/R8B_out)
    (add_net /relaysheet/Relais1)
    (add_net /relaysheet/Relais2)
    (add_net /relaysheet/Relais3)
    (add_net /relaysheet/Relais4)
    (add_net /relaysheet/Relais5)
    (add_net /relaysheet/Relais6)
    (add_net /relaysheet/Relais7)
    (add_net /relaysheet/Relais8)
    (add_net GNDA)
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD2D653)
    (at 25.4 109.22 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (path /5CD2A3B0)
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x09_Male (at 0 22.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 10.16 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 22.1) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 22.1) (end 1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 21.65) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 21.59) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 21.59) (end -1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /relaysheet/Relais1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /relaysheet/Relais2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /relaysheet/Relais3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /relaysheet/Relais4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /relaysheet/Relais8))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD2D670)
    (at 138.43 88.9)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (path /5CD2A41C)
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x09_Male (at 0 22.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 21.59) (end -1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 21.59) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 21.65) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 22.1) (end 1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 22.1) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 10.16 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D6D0)
    (at 183.85 57.15 90)
    (path /5CD2BD35/5CD2D6AA)
    (fp_text reference U1 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 12 /relaysheet/R1A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 11 /relaysheet/R1B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 1 /relaysheet/Relais1))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2F79B)
    (at 166.67 57.15 90)
    (path /5CD2BD35/5CD30362)
    (fp_text reference U2 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 17 /relaysheet/R2A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 16 /relaysheet/R2B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 4 /relaysheet/Relais2))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D700)
    (at 148.59 57.15 90)
    (path /5CD2BD35/5CD316D2)
    (fp_text reference U3 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 20 /relaysheet/R3A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 21 /relaysheet/R3B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 6 /relaysheet/Relais3))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD30B02)
    (at 130.71 57.15 90)
    (path /5CD2BD35/5CD31724)
    (fp_text reference U4 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 8 /relaysheet/Relais4))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 25 /relaysheet/R4B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 24 /relaysheet/R4A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D730)
    (at 112.73 57.15 90)
    (path /5CD2BD35/5CD2FCCA)
    (fp_text reference U5 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 14 /relaysheet/R5B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 15 /relaysheet/R5A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D748)
    (at 95.25 57.15 90)
    (path /5CD2BD35/5CD3038B)
    (fp_text reference U6 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 19 /relaysheet/R6B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 18 /relaysheet/R6A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2DE4A)
    (at 74.93 57.15 90)
    (path /5CD2BD35/5CD316FB)
    (fp_text reference U7 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 22 /relaysheet/R7B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 23 /relaysheet/R7A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD30EC6)
    (at 56.85 57.15 90)
    (path /5CD2BD35/5CD3174D)
    (fp_text reference U8 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 9 /relaysheet/Relais8))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 27 /relaysheet/R8B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 26 /relaysheet/R8A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_2x16_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD2ECFD)
    (at 111.76 73.66 270)
    (descr "Through hole straight pin header, 2x16, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x16 2.54mm double row")
    (path /5CE321D3)
    (fp_text reference J9 (at 1.27 -2.33 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x16_Odd_Even (at 1.27 40.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -1.27) (end 3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -1.27) (end 3.81 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 39.37) (end -1.27 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 39.37) (end -1.27 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 0) (end 0 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 39.43) (end 3.87 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.87 -1.33) (end 3.87 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 39.9) (end 4.35 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 39.9) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.27 19.05) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /relaysheet/R1A_out))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /relaysheet/R1B_out))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /relaysheet/R2A_out))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /relaysheet/R2B_out))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /relaysheet/R3A_out))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /relaysheet/R3B_out))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /relaysheet/R4A_out))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /relaysheet/R4B_out))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /relaysheet/R5A_out))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /relaysheet/R5B_out))
    (pad 20 thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 21 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /relaysheet/R6A_out))
    (pad 22 thru_hole oval (at 2.54 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 23 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /relaysheet/R6B_out))
    (pad 24 thru_hole oval (at 2.54 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 25 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /relaysheet/R7A_out))
    (pad 26 thru_hole oval (at 2.54 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 27 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /relaysheet/R7B_out))
    (pad 28 thru_hole oval (at 2.54 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 29 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /relaysheet/R8A_out))
    (pad 30 thru_hole oval (at 2.54 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 31 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /relaysheet/R8B_out))
    (pad 32 thru_hole oval (at 2.54 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F417)
    (at 180.34 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD2E7CE)
    (fp_text reference D1 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /relaysheet/Relais1))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F435)
    (at 162.56 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD3037D)
    (fp_text reference D2 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /relaysheet/Relais2))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F453)
    (at 144.78 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD316ED)
    (fp_text reference D3 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /relaysheet/Relais3))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD30AAF)
    (at 127 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD3173F)
    (fp_text reference D4 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /relaysheet/Relais4))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F48F)
    (at 109.22 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD2FCE5)
    (fp_text reference D5 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F4AD)
    (at 91.44 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD303A6)
    (fp_text reference D6 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F4CB)
    (at 71.12 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD31716)
    (fp_text reference D7 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD30E70)
    (at 53.34 66.04)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD31768)
    (fp_text reference D8 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /relaysheet/Relais8))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD31892)
    (at 16.51 41.91)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (path /5CE859BA)
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x10 (at 0 25.19) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.13) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 24.19) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 24.65) (end 1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 24.65) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 12.7 78.74) (end 12.7 12.7) (layer F.SilkS) (width 0.2))
  (gr_line (start 243.84 78.74) (end 12.7 78.74) (layer F.SilkS) (width 0.2))
  (gr_line (start 243.84 12.7) (end 243.84 78.74) (layer F.SilkS) (width 0.2))
  (gr_line (start 12.7 12.7) (end 243.84 12.7) (layer F.SilkS) (width 0.2) (tstamp 5CD2E5DF))

  (segment (start 52.07 54.61) (end 51.1 54.61) (width 1) (layer F.Cu) (net 13) (tstamp 5CD30EAD) (status 30))
  (segment (start 59.16 59.69) (end 58.42 58.95) (width 1) (layer F.Cu) (net 13))
  (segment (start 61.63 59.69) (end 59.16 59.69) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 58.42 58.95) (end 58.42 17.78) (width 1) (layer F.Cu) (net 13))
  (segment (start 54.54 59.69) (end 55.88 58.35) (width 1) (layer F.Cu) (net 13))
  (segment (start 52.07 59.69) (end 54.54 59.69) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 55.88 58.35) (end 55.88 17.78) (width 1) (layer F.Cu) (net 13))
  (segment (start 72.62 59.69) (end 73.66 58.65) (width 1) (layer F.Cu) (net 13))
  (segment (start 70.15 59.69) (end 72.62 59.69) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 73.66 58.65) (end 73.66 17.78) (width 1) (layer F.Cu) (net 13))
  (segment (start 77.24 59.69) (end 76.2 58.65) (width 1) (layer F.Cu) (net 13))
  (segment (start 79.71 59.69) (end 77.24 59.69) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 76.2 58.65) (end 76.2 17.78) (width 1) (layer F.Cu) (net 13))
  (segment (start 67.179999 54.109999) (end 67.179999 49.660001) (width 1) (layer F.Cu) (net 13))
  (segment (start 67.68 54.61) (end 67.179999 54.109999) (width 1) (layer F.Cu) (net 13))
  (segment (start 70.15 54.61) (end 67.68 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 67.179999 49.660001) (end 68.58 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 68.58 48.26) (end 71.12 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 71.12 48.26) (end 71.12 17.78) (width 1) (layer F.Cu) (net 13))
  (segment (start 64.600001 54.109999) (end 64.600001 49.360001) (width 1) (layer F.Cu) (net 13))
  (segment (start 64.1 54.61) (end 64.600001 54.109999) (width 1) (layer F.Cu) (net 13))
  (segment (start 61.63 54.61) (end 64.1 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 64.600001 49.360001) (end 63.5 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 63.5 48.26) (end 60.96 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 60.96 48.26) (end 60.96 17.78) (width 1) (layer F.Cu) (net 13))
  (segment (start 49.099999 54.109999) (end 49.099999 49.960001) (width 1) (layer F.Cu) (net 13))
  (segment (start 49.6 54.61) (end 49.099999 54.109999) (width 1) (layer F.Cu) (net 13))
  (segment (start 52.07 54.61) (end 49.6 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 49.099999 49.960001) (end 50.8 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 50.8 48.26) (end 53.34 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 53.34 48.26) (end 53.34 17.78) (width 1) (layer F.Cu) (net 13))
  (segment (start 82.680001 53.770001) (end 82.680001 49.660001) (width 1) (layer F.Cu) (net 13))
  (segment (start 81.840002 54.61) (end 82.680001 53.770001) (width 1) (layer F.Cu) (net 13))
  (segment (start 79.71 54.61) (end 81.840002 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 82.680001 49.660001) (end 81.28 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 81.28 48.26) (end 78.74 48.26) (width 1) (layer F.Cu) (net 13))
  (segment (start 78.74 48.26) (end 78.74 17.78) (width 1) (layer F.Cu) (net 13))

)
