(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 134)
    (zones 0)
    (modules 20)
    (nets 28)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /relaysheet/Relais1)
  (net 2 +9V)
  (net 3 /relaysheet/Relais5)
  (net 4 /relaysheet/Relais2)
  (net 5 /relaysheet/Relais6)
  (net 6 /relaysheet/Relais3)
  (net 7 /relaysheet/Relais7)
  (net 8 /relaysheet/Relais4)
  (net 9 /relaysheet/Relais8)
  (net 10 GNDA)
  (net 11 /relaysheet/R1B_out)
  (net 12 /relaysheet/R1A_out)
  (net 13 /relaysheet/R1A_NC)
  (net 14 /relaysheet/R5B_out)
  (net 15 /relaysheet/R5A_out)
  (net 16 /relaysheet/R2B_out)
  (net 17 /relaysheet/R2A_out)
  (net 18 /relaysheet/R6A_out)
  (net 19 /relaysheet/R6B_out)
  (net 20 /relaysheet/R3A_out)
  (net 21 /relaysheet/R3B_out)
  (net 22 /relaysheet/R7B_out)
  (net 23 /relaysheet/R7A_out)
  (net 24 /relaysheet/R4A_out)
  (net 25 /relaysheet/R4B_out)
  (net 26 /relaysheet/R8A_out)
  (net 27 /relaysheet/R8B_out)

  (net_class Default "This is the default net class."
    (clearance 1)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net /relaysheet/R1A_NC)
    (add_net /relaysheet/R1A_out)
    (add_net /relaysheet/R1B_out)
    (add_net /relaysheet/R2A_out)
    (add_net /relaysheet/R2B_out)
    (add_net /relaysheet/R3A_out)
    (add_net /relaysheet/R3B_out)
    (add_net /relaysheet/R4A_out)
    (add_net /relaysheet/R4B_out)
    (add_net /relaysheet/R5A_out)
    (add_net /relaysheet/R5B_out)
    (add_net /relaysheet/R6A_out)
    (add_net /relaysheet/R6B_out)
    (add_net /relaysheet/R7A_out)
    (add_net /relaysheet/R7B_out)
    (add_net /relaysheet/R8A_out)
    (add_net /relaysheet/R8B_out)
    (add_net /relaysheet/Relais1)
    (add_net /relaysheet/Relais2)
    (add_net /relaysheet/Relais3)
    (add_net /relaysheet/Relais4)
    (add_net /relaysheet/Relais5)
    (add_net /relaysheet/Relais6)
    (add_net /relaysheet/Relais7)
    (add_net /relaysheet/Relais8)
    (add_net GNDA)
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD2D653)
    (at 142.24 76.2 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (path /5CD2A3B0)
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x09_Male (at 0 22.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 10.16 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 22.1) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 22.1) (end 1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 21.65) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 21.59) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 21.59) (end -1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /relaysheet/Relais1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /relaysheet/Relais2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /relaysheet/Relais3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /relaysheet/Relais4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /relaysheet/Relais8))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD2D670)
    (at 138.43 88.9)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (path /5CD2A41C)
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x09_Male (at 0 22.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 21.59) (end -1.27 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 21.59) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 21.65) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 22.1) (end 1.8 22.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 22.1) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 10.16 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D6D0)
    (at 158.45 52.07 90)
    (path /5CD2BD35/5CD2D6AA)
    (fp_text reference U1 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 12 /relaysheet/R1A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 11 /relaysheet/R1B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 1 /relaysheet/Relais1))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2F79B)
    (at 141.27 52.07 90)
    (path /5CD2BD35/5CD30362)
    (fp_text reference U2 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 17 /relaysheet/R2A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 16 /relaysheet/R2B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 4 /relaysheet/Relais2))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D700)
    (at 123.19 52.07 90)
    (path /5CD2BD35/5CD316D2)
    (fp_text reference U3 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 20 /relaysheet/R3A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 21 /relaysheet/R3B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 6 /relaysheet/Relais3))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD30B02)
    (at 105.31 52.07 90)
    (path /5CD2BD35/5CD31724)
    (fp_text reference U4 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 8 /relaysheet/Relais4))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 25 /relaysheet/R4B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 24 /relaysheet/R4A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D730)
    (at 87.33 52.07 90)
    (path /5CD2BD35/5CD2FCCA)
    (fp_text reference U5 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 14 /relaysheet/R5B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 15 /relaysheet/R5A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D748)
    (at 69.85 52.07 90)
    (path /5CD2BD35/5CD3038B)
    (fp_text reference U6 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 19 /relaysheet/R6B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 18 /relaysheet/R6A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2DE4A)
    (at 49.53 52.07 90)
    (path /5CD2BD35/5CD316FB)
    (fp_text reference U7 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 22 /relaysheet/R7B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 23 /relaysheet/R7A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD30EC6)
    (at 31.45 52.07 90)
    (path /5CD2BD35/5CD3174D)
    (fp_text reference U8 (at 10.16 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 9 /relaysheet/Relais8))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 27 /relaysheet/R8B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 26 /relaysheet/R8A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_2x16_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD2ECFD)
    (at 111.76 73.66 270)
    (descr "Through hole straight pin header, 2x16, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x16 2.54mm double row")
    (path /5CE321D3)
    (fp_text reference J9 (at 1.27 -2.33 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x16_Odd_Even (at 1.27 40.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -1.27) (end 3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -1.27) (end 3.81 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 39.37) (end -1.27 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 39.37) (end -1.27 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 0) (end 0 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 39.43) (end 3.87 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.87 -1.33) (end 3.87 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 39.9) (end 4.35 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 39.9) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.27 19.05) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /relaysheet/R1B_out))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /relaysheet/R1A_out))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /relaysheet/R2B_out))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /relaysheet/R2A_out))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /relaysheet/R3B_out))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /relaysheet/R3A_out))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /relaysheet/R4B_out))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /relaysheet/R4A_out))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /relaysheet/R5B_out))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /relaysheet/R5A_out))
    (pad 20 thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 21 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /relaysheet/R6B_out))
    (pad 22 thru_hole oval (at 2.54 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 23 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /relaysheet/R6A_out))
    (pad 24 thru_hole oval (at 2.54 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 25 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /relaysheet/R7B_out))
    (pad 26 thru_hole oval (at 2.54 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 27 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /relaysheet/R7A_out))
    (pad 28 thru_hole oval (at 2.54 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 29 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /relaysheet/R8B_out))
    (pad 30 thru_hole oval (at 2.54 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 31 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /relaysheet/R8A_out))
    (pad 32 thru_hole oval (at 2.54 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F417)
    (at 154.94 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD2E7CE)
    (fp_text reference D1 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /relaysheet/Relais1))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F435)
    (at 137.16 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD3037D)
    (fp_text reference D2 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /relaysheet/Relais2))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F453)
    (at 119.38 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD316ED)
    (fp_text reference D3 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /relaysheet/Relais3))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD30AAF)
    (at 101.6 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD3173F)
    (fp_text reference D4 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /relaysheet/Relais4))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F48F)
    (at 83.82 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD2FCE5)
    (fp_text reference D5 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F4AD)
    (at 66.04 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD303A6)
    (fp_text reference D6 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F4CB)
    (at 45.72 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD31716)
    (fp_text reference D7 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD30E70)
    (at 27.94 60.96)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD31768)
    (fp_text reference D8 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /relaysheet/Relais8))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD31892)
    (at 17.78 17.78)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (path /5CE859BA)
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x10 (at 0 25.19) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.13) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 24.19) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 24.65) (end 1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 24.65) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 12.7 78.74) (end 12.7 12.7) (layer F.SilkS) (width 0.2))
  (gr_line (start 243.84 78.74) (end 12.7 78.74) (layer F.SilkS) (width 0.2))
  (gr_line (start 243.84 12.7) (end 243.84 78.74) (layer F.SilkS) (width 0.2))
  (gr_line (start 12.7 12.7) (end 243.84 12.7) (layer F.SilkS) (width 0.2) (tstamp 5CD2E5DF))

  (segment (start 162.56 57.82) (end 163.23 57.15) (width 1) (layer F.Cu) (net 1) (status 20))
  (segment (start 162.56 60.96) (end 162.56 57.82) (width 1) (layer F.Cu) (net 1) (status 10))
  (segment (start 27.94 58.42) (end 26.67 57.15) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 27.94 60.96) (end 27.94 58.42) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 45.72 58.12) (end 44.75 57.15) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 45.72 60.96) (end 45.72 58.12) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 66.04 58.12) (end 65.07 57.15) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 66.04 60.96) (end 66.04 58.12) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 83.82 58.42) (end 82.55 57.15) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 83.82 60.96) (end 83.82 58.42) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 101.6 58.22) (end 100.53 57.15) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 101.6 60.96) (end 101.6 58.22) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 119.38 58.12) (end 118.41 57.15) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 119.38 60.96) (end 119.38 58.12) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 154.94 58.42) (end 153.67 57.15) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 154.94 60.96) (end 154.94 58.42) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 91.44 57.82) (end 92.11 57.15) (width 1) (layer F.Cu) (net 3) (status 20))
  (segment (start 91.44 60.96) (end 91.44 57.82) (width 1) (layer F.Cu) (net 3) (status 10))
  (segment (start 73.66 58.12) (end 74.63 57.15) (width 1) (layer F.Cu) (net 5) (status 20))
  (segment (start 73.66 60.96) (end 73.66 58.12) (width 1) (layer F.Cu) (net 5) (status 10))
  (segment (start 127 58.12) (end 127.97 57.15) (width 1) (layer F.Cu) (net 6) (status 20))
  (segment (start 127 60.96) (end 127 58.12) (width 1) (layer F.Cu) (net 6) (status 10))
  (segment (start 53.34 58.12) (end 54.31 57.15) (width 1) (layer F.Cu) (net 7) (status 20))
  (segment (start 53.34 60.96) (end 53.34 58.12) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 109.22 58.02) (end 110.09 57.15) (width 1) (layer F.Cu) (net 8) (status 20))
  (segment (start 109.22 60.96) (end 109.22 58.02) (width 1) (layer F.Cu) (net 8) (status 10))
  (segment (start 35.56 57.82) (end 36.23 57.15) (width 1) (layer F.Cu) (net 9) (status 20))
  (segment (start 35.56 60.96) (end 35.56 57.82) (width 1) (layer F.Cu) (net 9) (status 10))
  (segment (start 26.67 49.53) (end 25.7 49.53) (width 1) (layer F.Cu) (net 13) (tstamp 5CD30EAD) (status 30))
  (segment (start 25.4 43.18) (end 27.94 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 26.67 49.53) (end 24.2 49.53) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 24.2 49.53) (end 23.699999 49.029999) (width 1) (layer F.Cu) (net 13))
  (segment (start 23.699999 49.029999) (end 23.699999 44.880001) (width 1) (layer F.Cu) (net 13))
  (segment (start 23.699999 44.880001) (end 25.4 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 30.48 53.27) (end 30.48 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 29.14 54.61) (end 30.48 53.27) (width 1) (layer F.Cu) (net 13))
  (segment (start 26.67 54.61) (end 29.14 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 33.02 53.87) (end 33.02 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 33.76 54.61) (end 33.02 53.87) (width 1) (layer F.Cu) (net 13))
  (segment (start 36.23 54.61) (end 33.76 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 35.56 43.18) (end 35.56 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 38.1 43.18) (end 35.56 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 36.23 49.53) (end 38.7 49.53) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 38.7 49.53) (end 39.200001 49.029999) (width 1) (layer F.Cu) (net 13))
  (segment (start 39.200001 49.029999) (end 39.200001 44.280001) (width 1) (layer F.Cu) (net 13))
  (segment (start 39.200001 44.280001) (end 38.1 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 43.18 43.18) (end 45.72 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 45.72 43.18) (end 45.72 20.32) (width 1) (layer F.Cu) (net 13))
  (segment (start 44.75 49.53) (end 42.28 49.53) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 41.779999 49.029999) (end 41.779999 44.580001) (width 1) (layer F.Cu) (net 13))
  (segment (start 42.28 49.53) (end 41.779999 49.029999) (width 1) (layer F.Cu) (net 13))
  (segment (start 41.779999 44.580001) (end 43.18 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 48.26 53.57) (end 48.26 20.32) (width 1) (layer F.Cu) (net 13))
  (segment (start 47.22 54.61) (end 48.26 53.57) (width 1) (layer F.Cu) (net 13))
  (segment (start 44.75 54.61) (end 47.22 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 50.8 53.57) (end 50.8 20.32) (width 1) (layer F.Cu) (net 13))
  (segment (start 51.84 54.61) (end 50.8 53.57) (width 1) (layer F.Cu) (net 13))
  (segment (start 54.31 54.61) (end 51.84 54.61) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 53.34 43.18) (end 53.34 20.32) (width 1) (layer F.Cu) (net 13))
  (segment (start 55.88 43.18) (end 53.34 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 56.440002 49.53) (end 57.280001 48.690001) (width 1) (layer F.Cu) (net 13))
  (segment (start 57.280001 48.690001) (end 57.280001 44.580001) (width 1) (layer F.Cu) (net 13))
  (segment (start 54.31 49.53) (end 56.440002 49.53) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 57.280001 44.580001) (end 55.88 43.18) (width 1) (layer F.Cu) (net 13))
  (segment (start 17.78 38.1) (end 27.94 38.1) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 35.56) (end 27.94 35.56) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 33.02) (end 27.94 33.02) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 30.48) (end 27.94 30.48) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 27.94) (end 27.94 27.94) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 25.4) (end 27.94 25.4) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 22.86) (end 27.94 22.86) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 20.32) (end 27.94 20.32) (width 1) (layer B.Cu) (net 13) (status 10))
  (segment (start 27.94 43.18) (end 27.94 20.32) (width 1) (layer F.Cu) (net 13))
  (segment (start 27.94 38.1) (end 165.1 38.1) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CDC))
  (via (at 27.94 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 35.56) (end 33.02 35.56) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CDE))
  (via (at 27.94 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 33.02) (end 30.48 33.02) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CE0))
  (via (at 27.94 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 30.48) (end 30.48 30.48) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CE2))
  (via (at 27.94 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 27.94) (end 30.48 27.94) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CE4))
  (via (at 27.94 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 25.4) (end 30.48 25.4) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CE6))
  (via (at 27.94 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 22.86) (end 165.1 22.86) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CE8))
  (via (at 27.94 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 20.32) (end 165.1 20.32) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31CEA))
  (via (at 27.94 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 30.48 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 22.86) (end 30.48 20.32) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31CEE))
  (via (at 30.48 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 33.02 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 22.86) (end 33.02 20.32) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31CF2))
  (via (at 33.02 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 35.56 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 22.86) (end 35.56 20.32) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31CF6))
  (via (at 35.56 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 25.4) (end 35.56 22.86) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31CF8))
  (via (at 35.56 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 27.94) (end 35.56 25.4) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31CFA))
  (via (at 35.56 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 30.48) (end 35.56 27.94) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31CFC))
  (via (at 35.56 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 33.02) (end 35.56 30.48) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31CFE))
  (via (at 35.56 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 35.56) (end 35.56 33.02) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D00))
  (via (at 35.56 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 38.1) (end 35.56 35.56) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D02))
  (via (at 35.56 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 38.1) (end 33.02 33.02) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D04))
  (via (at 33.02 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 35.56) (end 165.1 35.56) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31D06))
  (via (at 33.02 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 35.56) (end 30.48 22.86) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D08))
  (via (at 30.48 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 38.1) (end 30.48 35.56) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D0A))
  (via (at 30.48 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 33.02) (end 165.1 33.02) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31D0C))
  (via (at 30.48 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 30.48) (end 165.1 30.48) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31D0E))
  (via (at 33.02 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 33.02) (end 33.02 27.94) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D10))
  (via (at 33.02 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 30.48) (end 33.02 30.48) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31D12))
  (via (at 30.48 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 27.94) (end 165.1 27.94) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31D14))
  (via (at 30.48 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 25.4) (end 165.1 25.4) (width 1) (layer B.Cu) (net 13) (tstamp 5CD31D16))
  (via (at 30.48 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 25.4) (end 33.02 22.86) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D18))
  (via (at 33.02 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 27.94) (end 33.02 25.4) (width 1) (layer F.Cu) (net 13) (tstamp 5CD31D1A))
  (via (at 33.02 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))

)
