(export (version D)
  (design
    (source /media/fisch/HDD/Projects/mixer/mixersupply/mixersupply.sch)
    (date "Di 07 Mai 2019 17:56:31 CEST")
    (tool "Eeschema 5.0.2-bee76a0~70~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title Mixersupply)
        (company)
        (rev 1)
        (date 2018-10-19)
        (source mixersupply.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref F1)
      (value "Fuse 1.6A T")
      (footprint mixersupply_fuse:Fuseholder0520)
      (datasheet ~)
      (libsource (lib Device) (part Fuse) (description Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA8F401))
    (comp (ref D5)
      (value DIODE)
      (footprint Diode_THT:D_A-405_P12.70mm_Horizontal)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA90880))
    (comp (ref Cp2)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA9461B))
    (comp (ref Cn2)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA94683))
    (comp (ref Cn6)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA946CF))
    (comp (ref Cp6)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA9471D))
    (comp (ref DB9V1)
      (value "Diode Bridge")
      (footprint Diode_THT:Diode_Bridge_16.7x16.7x6.3mm_P10.8mm)
      (datasheet ~)
      (libsource (lib Device) (part D_Bridge_+A-A) (description "Diode bridge, +ve/AC/-ve/AC"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA99D11))
    (comp (ref U1)
      (value LM7805_TO220)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.fairchildsemi.com/ds/LM/LM7805.pdf)
      (libsource (lib Regulator_Linear) (part LM7805_TO220) (description "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA9BAA4))
    (comp (ref Cl1)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA9DCA8))
    (comp (ref Cl3)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BA9DCFE))
    (comp (ref J3)
      (value "Conn Front Power LED")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAAAD4C))
    (comp (ref RLED_PWR1)
      (value 220)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAAAFB0))
    (comp (ref Q1)
      (value BC337)
      (footprint Package_TO_SOT_THT:TO-92_Wide)
      (datasheet ~)
      (libsource (lib Device) (part Q_NPN_CBE) (description "NPN transistor, collector/base/emitter"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAB4103))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAC5B2A))
    (comp (ref C10)
      (value 220u)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAC5BAC))
    (comp (ref Cp3)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BACFEFE))
    (comp (ref Cn3)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAD21EE))
    (comp (ref Cn1)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAD2240))
    (comp (ref Cp1)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAD229A))
    (comp (ref J1)
      (value "230V In")
      (footprint mixersupply_connectors:AC_Connector)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAE5D12))
    (comp (ref F2)
      (value "1A T")
      (footprint mixersupply_fuse:Fuseholder0520)
      (datasheet ~)
      (libsource (lib Device) (part Fuse) (description Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAEC65A))
    (comp (ref F3)
      (value "1A T")
      (footprint mixersupply_fuse:Fuseholder0520)
      (datasheet ~)
      (libsource (lib Device) (part Fuse) (description Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAEC8A6))
    (comp (ref R3)
      (value 820)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAEC912))
    (comp (ref Cp5)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAEC9BC))
    (comp (ref Cn5)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAECA18))
    (comp (ref Cp4)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAF9575))
    (comp (ref Cn4)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAF961B))
    (comp (ref Cp7)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAF9689))
    (comp (ref Cn7)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAF978F))
    (comp (ref R4)
      (value 820)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB078D6))
    (comp (ref DLED_+12V1)
      (value LED)
      (footprint LED_THT:LED_D3.0mm_Clear)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB079C7))
    (comp (ref DLED_-12V1)
      (value LED)
      (footprint LED_THT:LED_D3.0mm_Clear)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB07DFF))
    (comp (ref RLED_5V1)
      (value 220)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB2349E))
    (comp (ref DLED_5V1)
      (value LED)
      (footprint LED_THT:LED_D3.0mm_Clear)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB23554))
    (comp (ref D2)
      (value 1N4001)
      (footprint Diode_THT:D_A-405_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC27385))
    (comp (ref D4)
      (value 1N4001)
      (footprint Diode_THT:D_A-405_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC27515))
    (comp (ref D1)
      (value 1N4001)
      (footprint Diode_THT:D_A-405_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC2762F))
    (comp (ref D3)
      (value 1N4001)
      (footprint Diode_THT:D_A-405_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC2778D))
    (comp (ref C5)
      (value 10n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC7C419))
    (comp (ref C2)
      (value 10n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC7C4B3))
    (comp (ref C3)
      (value 10n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC7C541))
    (comp (ref C4)
      (value 10n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC7C617))
    (comp (ref R1)
      (value 1k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BCC3BD9))
    (comp (ref J2)
      (value "PWR Switch")
      (footprint mixersupply_connectors:2Pin_8mm_w_clipconnector)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD2B533))
    (comp (ref C1)
      (value 10n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD527B0))
    (comp (ref Cl2)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD62732))
    (comp (ref Cl4)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD8B775))
    (comp (ref RV1)
      (value Varistor)
      (footprint Varistor:RV_Disc_D7mm_W3.4mm_P5mm)
      (datasheet ~)
      (libsource (lib Device) (part Varistor) (description "Voltage dependent resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BDC383D))
    (comp (ref J6)
      (value "Transformator Primary")
      (footprint mixersupply_connectors:2Pin_8mm_w_clipconnector)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC67AD5))
    (comp (ref J7)
      (value Transforer_15VAC)
      (footprint mixersupply_connectors:3Pin_4mm_w_clipconnector)
      (datasheet ~)
      (fields
        (field (name Notes) "Red, Black, Red"))
      (libsource (lib Connector) (part Conn_01x03_Male) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC8CF2E))
    (comp (ref C25)
      (value "203M SF 250V AC")
      (footprint Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P10.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BCEF457))
    (comp (ref U2)
      (value LM7815_TO220)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.fairchildsemi.com/ds/LM/LM7805.pdf)
      (libsource (lib Regulator_Linear) (part LM7815_TO220) (description "Positive 1A 35V Linear Regulator, Fixed Output 15V, TO-220"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD031A3))
    (comp (ref U3)
      (value LM7915_TO220)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.fairchildsemi.com/ds/LM/LM7905.pdf)
      (libsource (lib Regulator_Linear) (part LM7915_TO220) (description "Negative 1A 35V Linear Regulator, Fixed Output 15V, TO-220"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD0330F))
    (comp (ref K1)
      (value "DEG SDT-S-105LMR")
      (footprint "mixersupply_relay:Relais DEG SDT-S-105LMR")
      (datasheet http://gfinder.findernet.com/assets/Series/355/S32EN.pdf)
      (libsource (lib Relay) (part FINDER-32.21-x300) (description "FINDER 32.21-x300, Single Pole Relay SPST-NO, 6A"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD04C3D))
    (comp (ref R5)
      (value 100k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BCA7585))
    (comp (ref TH1)
      (value Thermistor_NTC)
      (footprint Varistor:RV_Disc_D21.5mm_W4.8mm_P10mm)
      (datasheet ~)
      (libsource (lib Device) (part Thermistor_NTC) (description "Temperature dependent resistor, negative temperature coefficient"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BCBFCA3))
    (comp (ref J5)
      (value "+-15V Out")
      (footprint Connector_JST:JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06_Male) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD7A1B1))
    (comp (ref J4)
      (value "5V Out")
      (footprint Connector_JST:JST_XH_B05B-XH-A_1x05_P2.50mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x05_Male) (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BDBCC61))
    (comp (ref J8)
      (value "Transformer 9VAC")
      (footprint mixersupply_connectors:2Pin_8mm_w_clipconnector)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BD541E4)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x03_Male)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector) (part Conn_01x05_Male)
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib Connector) (part Conn_01x06_Male)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D)
      (description Diode)
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part D_Bridge_+A-A)
      (description "Diode bridge, +ve/AC/-ve/AC")
      (docs ~)
      (footprints
        (fp D*Bridge*)
        (fp D*Rectifier*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Bridge_+A-A))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name ~~) (type passive))
        (pin (num 3) (name -) (type passive))
        (pin (num 4) (name ~~) (type passive))))
    (libpart (lib Device) (part Fuse)
      (description Fuse)
      (docs ~)
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Q_NPN_CBE)
      (description "NPN transistor, collector/base/emitter")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NPN_CBE))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Thermistor_NTC)
      (description "Temperature dependent resistor, negative temperature coefficient")
      (docs ~)
      (footprints
        (fp *NTC*)
        (fp *Thermistor*)
        (fp PIN?ARRAY*)
        (fp bornier*)
        (fp *Terminal?Block*))
      (fields
        (field (name Reference) TH)
        (field (name Value) Thermistor_NTC))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Varistor)
      (description "Voltage dependent resistor")
      (docs ~)
      (footprints
        (fp RV_*)
        (fp Varistor*))
      (fields
        (field (name Reference) RV)
        (field (name Value) Varistor))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Regulator_Linear) (part LM7805_TO220)
      (aliases
        (alias LM7806_TO220)
        (alias LM7808_TO220)
        (alias LM7809_TO220)
        (alias LM7810_TO220)
        (alias LM7812_TO220)
        (alias LM7815_TO220)
        (alias LM7818_TO220)
        (alias LM7824_TO220)
        (alias LM78M05_TO220)
        (alias SPX2920U-3.3_TO220)
        (alias SPX2920U-5.0_TO220)
        (alias LF15_TO220)
        (alias LF18_TO220)
        (alias LF25_TO220)
        (alias LF33_TO220)
        (alias LF50_TO220)
        (alias LF60_TO220)
        (alias LF80_TO220)
        (alias LF85_TO220)
        (alias LF120_TO220)
        (alias LF47_TO220)
        (alias LF90_TO220)
        (alias LM341T-05_TO220)
        (alias LM341T-12_TO220)
        (alias LM341T-15_TO220)
        (alias LM2937xT))
      (description "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
      (docs http://www.fairchildsemi.com/ds/LM/LM7805.pdf)
      (footprints
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM7805_TO220)
        (field (name Footprint) Package_TO_SOT_THT:TO-220-3_Vertical))
      (pins
        (pin (num 1) (name VI) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name VO) (type power_out))))
    (libpart (lib Regulator_Linear) (part LM7905_TO220)
      (aliases
        (alias LM79M05_TO220)
        (alias LM79M12_TO220)
        (alias LM79M15_TO220)
        (alias LM7906_TO220)
        (alias LM7908_TO220)
        (alias LM7909_TO220)
        (alias LM7910_TO220)
        (alias LM7915_TO220)
        (alias LM7912_TO220)
        (alias LM7918_TO220)
        (alias LM7924_TO220)
        (alias MC79M05_TO220)
        (alias MC79M08_TO220)
        (alias MC79M12_TO220)
        (alias MC79M15_TO220))
      (description "Negative 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
      (docs http://www.fairchildsemi.com/ds/LM/LM7905.pdf)
      (footprints
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM7905_TO220)
        (field (name Footprint) Package_TO_SOT_THT:TO-220-3_Vertical))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VI) (type power_in))
        (pin (num 3) (name VO) (type power_out))))
    (libpart (lib Relay) (part FINDER-32.21-x300)
      (aliases
        (alias FINDER-36.11-4301)
        (alias RM50-xx21))
      (description "FINDER 32.21-x300, Single Pole Relay SPST-NO, 6A")
      (docs http://gfinder.findernet.com/assets/Series/355/S32EN.pdf)
      (footprints
        (fp Relay*SPST*Finder*32.21*x300*))
      (fields
        (field (name Reference) K)
        (field (name Value) FINDER-32.21-x300)
        (field (name Footprint) Relay_THT:Relay_SPST_Finder_32.21-x300))
      (pins
        (pin (num 11) (name ~) (type passive))
        (pin (num 14) (name ~) (type passive))
        (pin (num A1) (name ~) (type passive))
        (pin (num A2) (name ~) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/library/Regulator_Linear.lib))
    (library (logical Relay)
      (uri /usr/share/kicad/library/Relay.lib)))
  (nets
    (net (code 1) (name +5V)
      (node (ref D5) (pin 1))
      (node (ref RLED_PWR1) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref Cl3) (pin 1))
      (node (ref K1) (pin A1))
      (node (ref RLED_5V1) (pin 1))
      (node (ref J4) (pin 4))
      (node (ref Cl4) (pin 1))
      (node (ref J4) (pin 3))
      (node (ref R2) (pin 1)))
    (net (code 2) (name "Net-(F1-Pad2)")
      (node (ref J2) (pin 2))
      (node (ref F1) (pin 2)))
    (net (code 3) (name "Net-(F1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref F1) (pin 1)))
    (net (code 4) (name "Net-(F2-Pad2)")
      (node (ref F2) (pin 2))
      (node (ref J7) (pin 3)))
    (net (code 5) (name "Net-(F3-Pad2)")
      (node (ref F3) (pin 2))
      (node (ref J7) (pin 1)))
    (net (code 6) (name "Net-(J1-Pad2)")
      (node (ref RV1) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 7) (name "Net-(C25-Pad2)")
      (node (ref TH1) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref J6) (pin 2))
      (node (ref K1) (pin 11)))
    (net (code 8) (name "Net-(C2-Pad2)")
      (node (ref Cn3) (pin 2))
      (node (ref Cn1) (pin 2))
      (node (ref Cn2) (pin 2))
      (node (ref Cn4) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 9) (name "Net-(C2-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref F2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C3) (pin 2)))
    (net (code 10) (name "Net-(C3-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref Cp1) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref Cp2) (pin 1))
      (node (ref Cp4) (pin 1))
      (node (ref Cp3) (pin 1)))
    (net (code 11) (name "Net-(C10-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref C10) (pin 1)))
    (net (code 12) (name "Net-(D5-Pad2)")
      (node (ref J3) (pin 1))
      (node (ref D5) (pin 2))
      (node (ref K1) (pin A2))
      (node (ref Q1) (pin 1)))
    (net (code 13) (name "Net-(Q1-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref R1) (pin 2)))
    (net (code 14) (name "Net-(C4-Pad1)")
      (node (ref D4) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref F3) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref C5) (pin 2)))
    (net (code 15) (name /9VAC_2)
      (node (ref J8) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref DB9V1) (pin 2)))
    (net (code 16) (name /9VAC_1)
      (node (ref C1) (pin 2))
      (node (ref DB9V1) (pin 4))
      (node (ref J8) (pin 1)))
    (net (code 17) (name -15V)
      (node (ref Cn6) (pin 2))
      (node (ref Cn5) (pin 2))
      (node (ref J5) (pin 1))
      (node (ref J5) (pin 2))
      (node (ref Cn7) (pin 2))
      (node (ref DLED_-12V1) (pin 1))
      (node (ref U3) (pin 3)))
    (net (code 18) (name +15V)
      (node (ref Cp5) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref Cp6) (pin 1))
      (node (ref Cp7) (pin 1))
      (node (ref J5) (pin 6))
      (node (ref U2) (pin 3))
      (node (ref J5) (pin 5)))
    (net (code 19) (name "Net-(C25-Pad1)")
      (node (ref K1) (pin 14))
      (node (ref RV1) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref TH1) (pin 1))
      (node (ref C25) (pin 1)))
    (net (code 20) (name "Net-(J3-Pad2)")
      (node (ref RLED_PWR1) (pin 1))
      (node (ref J3) (pin 2)))
    (net (code 21) (name GNDA)
      (node (ref DLED_+12V1) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref J5) (pin 3))
      (node (ref U3) (pin 1))
      (node (ref Cp5) (pin 2))
      (node (ref Cn5) (pin 1))
      (node (ref Cp4) (pin 2))
      (node (ref Cn4) (pin 1))
      (node (ref Cp7) (pin 2))
      (node (ref Cn7) (pin 1))
      (node (ref J7) (pin 2))
      (node (ref Cp1) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref J5) (pin 4))
      (node (ref Cp6) (pin 2))
      (node (ref Cp2) (pin 2))
      (node (ref Cn2) (pin 1))
      (node (ref Cn6) (pin 1))
      (node (ref Cn1) (pin 1))
      (node (ref Cn3) (pin 1))
      (node (ref Cp3) (pin 2)))
    (net (code 22) (name /9V)
      (node (ref J4) (pin 5))
      (node (ref DB9V1) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref Cl1) (pin 1))
      (node (ref Cl2) (pin 1)))
    (net (code 23) (name "Net-(DLED_-12V1-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref DLED_-12V1) (pin 2)))
    (net (code 24) (name GNDD)
      (node (ref Q1) (pin 3))
      (node (ref DLED_5V1) (pin 1))
      (node (ref Cl2) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref Cl4) (pin 2))
      (node (ref Cl1) (pin 2))
      (node (ref Cl3) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref DB9V1) (pin 3))
      (node (ref J4) (pin 1)))
    (net (code 25) (name "Net-(DLED_+12V1-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref DLED_+12V1) (pin 2)))
    (net (code 26) (name "Net-(DLED_5V1-Pad2)")
      (node (ref DLED_5V1) (pin 2))
      (node (ref RLED_5V1) (pin 2)))))